IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
File name: "Project Number"
Time stamp: "2021-05-25T08:50:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.1.109 - Exporter 21.2.1.0 - Alternate UI 21.2.1.0"
Application: "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)"

People and organizations
  Person "moud308" of Organization (no name given)
  Owner history of Person "moud308" of Organization (no name given) | application "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)" | change NOCHANGE | created 1621896642 (2021-05-24T22:50:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 3 elements
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" | object type "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" | names: "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P:317512" | material: constituents "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" ("Brick, Common": "Brick, Common", "Fiberglass Batt": "Fiberglass Batt", "Concrete Masonry Units _Low Density": "Concrete Masonry Units _Low Density", "Plaster": "Plaster") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "Doors_ExtDbl_Flush:1810x2110mm" | object type "Doors_ExtDbl_Flush:1810x2110mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "Doors_ExtDbl_Flush:1810x2110mm:317532" | material: constituents "MaterialConstituentSet" ("Door - Handle": "Door - Handle", "Door - Frame/Mullion": "Door - Frame/Mullion", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" | object type "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" | FLOOR | names: "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC:317566" | material: constituents "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" ("Concrete, Sand/Cement Screed": "Concrete, Sand/Cement Screed", "Rigid insulation": "Rigid insulation", "Air": "Air", "Concrete Masonry, Floor Block": "Concrete Masonry, Floor Block", "Concrete, Precast": "Concrete, Precast") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon

Types
  IFCWALLTYPE "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" | STANDARD | 1 occurrence | material: constituents "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" ("Brick, Common": "Brick, Common", "Fiberglass Batt": "Fiberglass Batt", "Concrete Masonry Units _Low Density": "Concrete Masonry Units _Low Density", "Plaster": "Plaster") | property sets: Pset_WallCommon
  IFCDOORTYPE "Doors_ExtDbl_Flush:1810x2110mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Ironmongery": "Door - Handle", "Frame/Mullion": "Door - Frame/Mullion", "Threshold": "Door - Frame/Mullion", "Panel": "Door - Panel") | property sets: Doors_ExtDbl_Flush:1810x2110mm:317532, Doors_ExtDbl_Flush:1810x2110mm:317532:1, Pset_DoorCommon
  IFCSLABTYPE "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" | FLOOR | 1 occurrence | material: constituents "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" ("Concrete, Sand/Cement Screed": "Concrete, Sand/Cement Screed", "Rigid insulation": "Rigid insulation", "Air": "Air", "Concrete Masonry, Floor Block": "Concrete Masonry, Floor Block", "Concrete, Precast": "Concrete, Precast") | property sets: Pset_SlabCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCWALL)
    Reference = "Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCDOOR)
    Reference = "1810x2110mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCIDENTIFIER)
    ThermalTransmittance = 0.235926059936681 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.235926059936681 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1810x2110mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCIDENTIFIER)
    ThermalTransmittance = 0.117437608263296 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0.117437608263296 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Circle Head - Project Datum" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Doors_ExtDbl_Flush:1810x2110mm:317532 | predefined | on 1 type object
  Doors_ExtDbl_Flush:1810x2110mm:317532:1 | predefined | on 1 type object