IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
File name: "test.ifc"
Time stamp: "2020-03-16T15:44:45"
Preprocessor: "BSProLib (Ver:2020.3.0.15)"
Authorization: "-"

Units
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: DECI CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  PRESSUREUNIT: PASCAL
  VOLUMETRICFLOWRATEUNIT: derived
  LINEARVELOCITYUNIT: derived
  LENGTHUNIT: MILLI METRE
  POWERUNIT: WATT
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT

Spatial structure
IFCPROJECT "Demoproject" | description "Demoproject for MCREV"
  IFCSITE | latitude 61° 29′ 52.295837″ | longitude 23° 45′ 45.792388″ | elevation above sea level -0.
    IFCBUILDING "mc-building" | postal address (none given)
      IFCBUILDINGSTOREY "1. floor" | elevation 0.
        contains 5 elements
          4 x IFCBUILDINGELEMENTPROXY | PROVISIONFORSPACE | names: "Maintenance zone (Switchboard-0002_001)" | descriptions: "Maintenance zone (Switchboard)"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "Switchboard-0002_001" | names: "Switchboard-0002_001" | descriptions: "Switchboard" | property sets: Pset_ElectricalCostData, Pset_ElectricalDeviceCommon, MagiCAD Pset_Switchboard

Types
  IFCELECTRICDISTRIBUTIONBOARDTYPE "Switchboard-0002_001" | DISTRIBUTIONBOARD | 1 occurrence | description "Switchboard"

Property sets
  MagiCAD Pset_Project | properties | on 1 object (1 IFCPROJECT)
    Author = "Technical Services" (IFCTEXT)
    Authorization = "" (IFCTEXT)
    Organization = "MagiCAD Group" (IFCTEXT)
    Project description = "Demoproject for MCREV" (IFCTEXT)
    Project long name = "" (IFCTEXT)
    Project name = "Demoproject" (IFCTEXT)
    Project phase = "" (IFCTEXT)
  MagiCAD Pset_Site | properties | on 1 object (1 IFCSITE)
    Description = "" (IFCTEXT)
    Land title number = "" (IFCTEXT)
    Long name = "" (IFCTEXT)
    Name = "" (IFCTEXT)
    Reference elevation = 0.0000 (IFCREAL)
    Reference latitude = "61, 29, 52, 295837" (IFCTEXT)
    Reference longitude = "23, 45, 45, 792388" (IFCTEXT)
  MagiCAD Pset_Building | properties | on 1 object (1 IFCBUILDING)
    Address country = "" (IFCTEXT)
    Address description = "" (IFCTEXT)
    Address internal location = "" (IFCTEXT)
    Address line 1 = "" (IFCTEXT)
    Address line 2 = "" (IFCTEXT)
    Address postal box = "" (IFCTEXT)
    Address postal code = "" (IFCTEXT)
    Address region = "" (IFCTEXT)
    Address town = "" (IFCTEXT)
    Building description = "" (IFCTEXT)
    Building long name = "" (IFCTEXT)
    Building name = "" (IFCTEXT)
  MagiCAD Pset_Storey | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Description = "" (IFCTEXT)
    Name = "1. floor" (IFCTEXT)
  MagiCAD Pset_System | properties | on 1 object (1 IFCDISTRIBUTIONCIRCUIT)
    Code = "H2" (IFCTEXT)
    Description = "Main distribution systems" (IFCTEXT)
  Pset_ElectricalCostData | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONBOARD)
    CostCodeName = "Eldata Kode" (IFCTEXT)
    CostCodeValue = "" (IFCIDENTIFIER)
    CostQuantity = 1 (IFCINTEGER)
    CostUnit = "EA" (IFCTEXT)
    Location = "NOR" (IFCTEXT)
    ProductCodeName = "NS3420" (IFCTEXT)
    ProductCodeValue = "" (IFCIDENTIFIER)
    SystemCodeName = "NS3451" (IFCTEXT)
    SystemCodeValue = "H2" (IFCIDENTIFIER)
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONBOARD)
    IP_Code = "IP31" (IFCTEXT)
    NumberOfPoles = 3 (IFCINTEGER)
    PowerFactor = 1.0000 (IFCNORMALISEDRATIOMEASURE)
    RatedVoltage = 400.0000 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  MagiCAD Pset_Switchboard | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONBOARD)
    Active Power = 0.0000 (IFCPOWERMEASURE) [WATT]
    Circuit no = "1,1,4.1,4.2,5.1,5.2,5.3,6.1,6.2,6.3,7.1,7.2,7.3,8.1,20.1,20.2,20.3,21.2,21.3,22.1,22.2,22.3,23.1,23.2,23.3,24.1,24.2,24.3,25.1,25.2" (IFCTEXT)
    Circuit order no = "1,2,3" (IFCTEXT)
    EX_Code = "" (IFCTEXT)
    IP_Code = "IP31" (IFCTEXT)
    Installation code = "S" (IFCTEXT)
    Number of Poles = 3 (IFCINTEGER)
    O1 = "" (IFCTEXT)
    O2 = "" (IFCTEXT)
    Power Factor = 1.0000 (IFCNORMALISEDRATIOMEASURE)
    Supplying switchboard = "MS" (IFCTEXT)
    Switchboard code = "SB10.1" (IFCTEXT)
    System code = "H2" (IFCTEXT)
    User code = "02" (IFCTEXT)
    Voltage = 400.0000 (IFCELECTRICVOLTAGEMEASURE) [VOLT]