IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "ExchangeRequirement [Architecture, Structural, BuildingService]"
Description: "Comment [Comments]"
Description: "Comment [System: OpenBuildings Designer10.00.00.99 debug build Jan 7 2020 12:03:14]"
File name: "TFS 1067632 Elem 17878 Solid 1 RV"
Time stamp: "2020-01-07T13:47:31+03:00"
Author: "First Name Last Name"
Organization: "Organization Name"
Preprocessor: "ST-DEVELOPER v16.13"
Originating system: "OpenBuildings Designer10.00.00.99"
Authorization: "Administrator"
Application: "OpenBuildings Designer" version "10.00.00.99" identifier "ABD" by Organization "Bentley Systems Inc."

People and organizations
  Person "First Name" "Last Name" (roles: SUPPLIER; telecom address: telephone "Phone"; e-mail "E-Mail") of Organization "Organization Name" (postal address: "Address 1", "Address 2", "City/Town", "State/Region", "Postal Code", "Country")
  Owner history of Person "First Name" "Last Name" (roles: SUPPLIER; telecom address: telephone "Phone"; e-mail "E-Mail") of Organization "Organization Name" (postal address: "Address 1", "Address 2", "City/Town", "State/Region", "Postal Code", "Country") | application "OpenBuildings Designer" version "10.00.00.99" identifier "ABD" by Organization "Bentley Systems Inc." | created 1578394034 (2020-01-07T10:47:14Z) | last modified 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: foot (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  ABSORBEDDOSEUNIT: GRAY
  AMOUNTOFSUBSTANCEUNIT: MOLE
  DOSEEQUIVALENTUNIT: SIEVERT
  ELECTRICCAPACITANCEUNIT: FARAD
  ELECTRICCHARGEUNIT: COULOMB
  ELECTRICCONDUCTANCEUNIT: SIEMENS
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICRESISTANCEUNIT: OHM
  ELECTRICVOLTAGEUNIT: VOLT
  ENERGYUNIT: JOULE
  FORCEUNIT: NEWTON
  FREQUENCYUNIT: HERTZ
  ILLUMINANCEUNIT: LUX
  INDUCTANCEUNIT: HENRY
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  MAGNETICFLUXDENSITYUNIT: TESLA
  MAGNETICFLUXUNIT: WEBER
  MASSUNIT: GRAM
  PLANEANGLEUNIT: degree (conversion based)
  POWERUNIT: WATT
  PRESSUREUNIT: PASCAL
  RADIOACTIVITYUNIT: BECQUEREL
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  TIMEUNIT: SECOND
  ACCELERATIONUNIT: derived "(FOOT)/(SECOND^2)"
  ANGULARVELOCITYUNIT: derived "(DEGREE)/(SECOND)"
  CURVATUREUNIT: derived "(DEGREE)/(FOOT)"
  DYNAMICVISCOSITYUNIT: derived "(PASCAL)(SECOND)"
  HEATFLUXDENSITYUNIT: derived "(WATT)/(FOOT^2)"
  HEATINGVALUEUNIT: derived "(JOULE)/(GRAM)"
  INTEGERCOUNTRATEUNIT: derived "1/(SECOND)"
  IONCONCENTRATIONUNIT: derived "(GRAM)/(CUBIC_METRE)"
  ISOTHERMALMOISTURECAPACITYUNIT: derived "(CUBIC_METRE)/(GRAM)"
  KINEMATICVISCOSITYUNIT: derived "(SQUARE_METRE)/(SECOND)"
  LINEARFORCEUNIT: derived "(NEWTON)/(FOOT)"
  LINEARMOMENTUNIT: derived "(NEWTON)/(FOOT)"
  LINEARSTIFFNESSUNIT: derived "(NEWTON)/(FOOT)"
  LINEARVELOCITYUNIT: derived "(FOOT)/(SECOND)"
  LUMINOUSINTENSITYDISTRIBUTIONUNIT: derived "(CANDELA)/(LUMEN)"
  MASSDENSITYUNIT: derived "(GRAM)/(CUBIC_METRE)"
  MASSFLOWRATEUNIT: derived "(GRAM)/(SECOND)"
  MASSPERLENGTHUNIT: derived "(GRAM)/(FOOT)"
  MODULUSOFELASTICITYUNIT: derived "(NEWTON)/(SQUARE_METRE)"
  MODULUSOFLINEARSUBGRADEREACTIONUNIT: derived "(NEWTON)/(FOOT^2)"
  MODULUSOFROTATIONALSUBGRADEREACTIONUNIT: derived "(NEWTON)(FOOT)"
  MODULUSOFSUBGRADEREACTIONUNIT: derived "(NEWTON)/(CUBIC_METRE)"
  MOISTUREDIFFUSIVITYUNIT: derived "(CUBIC_METRE)/(SECOND)"
  MOLECULARWEIGHTUNIT: derived "(GRAM)/(MOLE)"
  PLANARFORCEUNIT: derived "(NEWTON)/(FOOT^2)"
  ROTATIONALFREQUENCYUNIT: derived "1/(SECOND)"
  ROTATIONALMASSUNIT: derived "(GRAM)(FOOT^2)"
  ROTATIONALSTIFFNESSUNIT: derived "(NEWTON)(FOOT)/(DEGREE)"
  SECTIONAREAINTEGRALUNIT: derived "(FOOT^5)"
  SECTIONMODULUSUNIT: derived "(FOOT^3)"
  SHEARMODULUSUNIT: derived "(NEWTON)/(SQUARE_METRE)"
  SOUNDPOWERUNIT: derived "(JOULE)/(SECOND)"
  SPECIFICHEATCAPACITYUNIT: derived "(NEWTON)/(GRAM)(KELVIN)"
  TEMPERATUREGRADIENTUNIT: derived "(KELVIN)/(FOOT)"
  THERMALADMITTANCEUNIT: derived "(WATT)/(SQUARE_METRE)(KELVIN)"

Spatial structure
IFCPROJECT "BuildingTemplate_US" | long name "BuildingTemplate_US" | description "BuildingTemplate_US"
  IFCSITE "Site 1" | long name "Site 1" | elevation above sea level 0. | postal address: "Site 1" | description "Site 1"
    IFCBUILDING "Bldg 1" | long name "Bldg 1" | reference height above sea level 0. | terrain above sea level 0. | postal address: "203 Rickenhouse Drive", "Madison", "35789", "US" | description "3 Story Building"
      IFCBUILDINGSTOREY "Floor 1" | long name "Floor 1" | elevation 0. | description "Tellers and loan offices"
        contains 1 element
          1 x IFCRAILING | type IFCRAILINGTYPE "Pipe Railing" | object type "Railing" | HANDRAIL | names: "Pipe Railing" | descriptions: "17878*Defect 1067632 rails!Design Model" | material: "Plastic - lt gray" | property sets: RailingQuantities

Types
  IFCRAILINGTYPE "Pipe Railing" | HANDRAIL | 1 occurrence | property sets: Railing_Application

Property sets
  Project | properties | on 1 object (1 IFCPROJECT)
    ProjectName = "BuildingTemplate_US" (IFCTEXT)
  Site | properties | on 1 object (1 IFCSITE)
    BuildingHeightLimit = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    SiteName = "Site 1" (IFCTEXT)
  RailingQuantities | properties | on 1 object (1 IFCRAILING)
    Balusters/Balusters1/@Balusters1Count = 0 (IFCINTEGER)
    Balusters/Balusters1/@Balusters1Length = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters1/@Balusters1TotalLength = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2Count = 0 (IFCINTEGER)
    Balusters/Balusters2/@Balusters2Length = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2TotalLength = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3Count = 0 (IFCINTEGER)
    Balusters/Balusters3/@Balusters3Length = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3TotalLength = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/CornerPost/@CornerPostCount = 3 (IFCINTEGER)
    Posts/CornerPost/@CornerPostLength = 3.4166666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/CornerPost/@CornerPostTotalLength = 10.25 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/EndPost/@EndPostCount = 1 (IFCINTEGER)
    Posts/EndPost/@EndPostLength = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/EndPost/@EndPostTotalLength = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/IntermediatePost1/@IntermediatePost1Count = 3 (IFCINTEGER)
    Posts/IntermediatePost1/@IntermediatePost1Length = 3.8045352568 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/IntermediatePost1/@IntermediatePost1TotalLength = 11.4136057703 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/MountingBracket/@MountingBracketCount = 0 (IFCINTEGER)
    Posts/MountingBracket/@MountingBracketLength = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/MountingBracket/@MountingBracketTotalLength = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/StartPost/@StartPostCount = 1 (IFCINTEGER)
    Posts/StartPost/@StartPostLength = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/StartPost/@StartPostTotalLength = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail1/@Rail1Length = 23.4055253237 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail2/@Rail2Length = 23.4055253237 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail3/@Rail3Length = 23.4055253237 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail4/@Rail4Length = 22.874913211 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail5/@Rail5Length = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail6/@Rail6Length = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    YearOfConstruction = "2006" (IFCLABEL)
  ArchBuilding | properties | on 1 object (1 IFCBUILDING)
    BuildingName = "Bldg 1" (IFCTEXT)
    YearConstructed = "2006" (IFCTEXT)
  ObjectIdentity | properties | on 1 object (1 IFCBUILDING)
    Description = "3 Story Building" (IFCTEXT)
  ObjectPostalAddress | properties | on 1 object (1 IFCBUILDING)
    Address1 = "203 Rickenhouse Drive" (IFCTEXT)
    City = "Madison" (IFCTEXT)
    Country = "US" (IFCTEXT)
    PostalCode = "35789" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    GrossAreaPlanned = 2229.67296 (IFCAREAMEASURE) [SQUARE_METRE]
    GrossPlannedArea = 2229.67296 (IFCAREAMEASURE) [SQUARE_METRE]
    NetAreaPlanned = 2229.67296 (IFCAREAMEASURE) [SQUARE_METRE]
    NetPlannedArea = 2229.67296 (IFCAREAMEASURE) [SQUARE_METRE]
  ArchFloor | properties | on 1 object (1 IFCBUILDINGSTOREY)
    ACSRotation = "0.00000000" (IFCTEXT)
    Annotation = TRUE (IFCBOOLEAN)
    ApproxLength = 200. (IFCLENGTHMEASURE) [foot (conversion based)]
    ApproxWidth = 120. (IFCLENGTHMEASURE) [foot (conversion based)]
    Description = "Tellers and loan offices" (IFCTEXT)
    FinishedFloorElevation = 0. (IFCREAL)
    FloorName = "Floor 1" (IFCTEXT)
    TypicalFloor = FALSE (IFCBOOLEAN)
    TypicalFloorBaseElevation = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    TypicalFloorHeight = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
  Floor | properties | on 1 object (1 IFCBUILDINGSTOREY)
    GrossArea = 2229.67296 (IFCAREAMEASURE) [SQUARE_METRE]
    NetArea = 2229.67296 (IFCAREAMEASURE) [SQUARE_METRE]
    OccupancyType = "Commercial" (IFCTEXT)
  StructuralFloorCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    issplicefloor = FALSE (IFCBOOLEAN)
  Railing_Application | properties | on 1 type object
    Balusters/Balusters1/@Balusters1BaseOffset = 0.41666666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters1/@Balusters1Name = "Pickets" (IFCTEXT)
    Balusters/Balusters1/@Balusters1PartDef = "Circulation::Balusters" (IFCLABEL)
    Balusters/Balusters1/@Balusters1Profile = "RECT1x1" (IFCTEXT)
    Balusters/Balusters1/@Balusters1ProfileType = "<none>" (IFCTEXT)
    Balusters/Balusters1/@Balusters1SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters1/@Balusters1Spacing = 0.33333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters1/@Balusters1SpacingType = "Max Spacing" (IFCTEXT)
    Balusters/Balusters1/@Balusters1Thickness = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters1/@Balusters1TopOffset = 3.4166666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2BaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2PartDef = "Circulation::Balusters" (IFCLABEL)
    Balusters/Balusters2/@Balusters2Profile = "RECT1x1" (IFCTEXT)
    Balusters/Balusters2/@Balusters2ProfileType = "<none>" (IFCTEXT)
    Balusters/Balusters2/@Balusters2SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2Spacing = 0.33333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2SpacingType = "Max Spacing" (IFCTEXT)
    Balusters/Balusters2/@Balusters2Thickness = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters2/@Balusters2TopOffset = 2.41666666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3BaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3PartDef = "Circulation::Balusters" (IFCLABEL)
    Balusters/Balusters3/@Balusters3Profile = "RECT1x1" (IFCTEXT)
    Balusters/Balusters3/@Balusters3ProfileType = "<none>" (IFCTEXT)
    Balusters/Balusters3/@Balusters3SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3Spacing = 1.41666666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3SpacingType = "Max Spacing" (IFCTEXT)
    Balusters/Balusters3/@Balusters3Thickness = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Balusters/Balusters3/@Balusters3TopOffset = 2.41666666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Ends/End/@EndName = "End" (IFCTEXT)
    Ends/End/@EndPartDef = "Circulation::Railing" (IFCLABEL)
    Ends/End/@EndSideOffset = 0.33333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Ends/End/@EndTopOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Ends/Start/@StartName = "Start" (IFCTEXT)
    Ends/Start/@StartPartDef = "Circulation::Railing" (IFCLABEL)
    Ends/Start/@StartSideOffset = 0.33333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Ends/Start/@StartTopOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    GenerateDrawingSymbols = TRUE (IFCBOOLEAN)
    Posts/CornerPost/@CornerPostBaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/CornerPost/@CornerPostName = "Corner Post" (IFCTEXT)
    Posts/CornerPost/@CornerPostPartDef = "Circulation::Posts" (IFCLABEL)
    Posts/CornerPost/@CornerPostProfile = "PIPE1-1/2XS" (IFCTEXT)
    Posts/CornerPost/@CornerPostProfileType = "Structural Section" (IFCTEXT)
    Posts/CornerPost/@CornerPostSideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/CornerPost/@CornerPostSpacing = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/CornerPost/@CornerPostTopOffset = 3.4166666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/EndPost/@EndPostBaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/EndPost/@EndPostName = "End Post" (IFCTEXT)
    Posts/EndPost/@EndPostPartDef = "Circulation::Posts" (IFCLABEL)
    Posts/EndPost/@EndPostProfile = "PIPE1-1/2XS" (IFCTEXT)
    Posts/EndPost/@EndPostProfileType = "Structural Section" (IFCTEXT)
    Posts/EndPost/@EndPostSideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/EndPost/@EndPostSpacing = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/EndPost/@EndPostTopOffset = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/IntermediatePost1/@IntermediatePost1BaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/IntermediatePost1/@IntermediatePost1Name = "Intermediate Post" (IFCTEXT)
    Posts/IntermediatePost1/@IntermediatePost1PartDef = "Circulation::Posts" (IFCLABEL)
    Posts/IntermediatePost1/@IntermediatePost1Profile = "PIPE1-1/2XS" (IFCTEXT)
    Posts/IntermediatePost1/@IntermediatePost1ProfileType = "Structural Section" (IFCTEXT)
    Posts/IntermediatePost1/@IntermediatePost1SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/IntermediatePost1/@IntermediatePost1Spacing = 4. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/IntermediatePost1/@IntermediatePost1SpacingType = "Max Spacing" (IFCTEXT)
    Posts/IntermediatePost1/@IntermediatePost1TopOffset = 3.4166666667 (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/MountingBracket/@MountingBracketBaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/MountingBracket/@MountingBracketProfileType = "<none>" (IFCTEXT)
    Posts/MountingBracket/@MountingBracketSideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/MountingBracket/@MountingBracketSpacing = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/MountingBracket/@MountingBracketSpacingType = "Max Spacing" (IFCTEXT)
    Posts/MountingBracket/@MountingBracketTopOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/StartPost/@StartPostBaseOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/StartPost/@StartPostName = "Start Post" (IFCTEXT)
    Posts/StartPost/@StartPostPartDef = "Circulation::Posts" (IFCLABEL)
    Posts/StartPost/@StartPostProfile = "PIPE1-1/2XS" (IFCTEXT)
    Posts/StartPost/@StartPostProfileType = "Structural Section" (IFCTEXT)
    Posts/StartPost/@StartPostSideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/StartPost/@StartPostSpacing = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Posts/StartPost/@StartPostTopOffset = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    RailingPartDef = "Circulation::Railing" (IFCLABEL)
    Rails/Rail1/@Rail1JoinMethod = "<none>" (IFCTEXT)
    Rails/Rail1/@Rail1Name = "Top" (IFCTEXT)
    Rails/Rail1/@Rail1PartDef = "Circulation::Railing" (IFCLABEL)
    Rails/Rail1/@Rail1Profile = "PIPE1-1/2XS" (IFCTEXT)
    Rails/Rail1/@Rail1ProfileType = "Structural Section" (IFCTEXT)
    Rails/Rail1/@Rail1SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail1/@Rail1TopOffset = 3.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail2/@Rail2JoinMethod = "<none>" (IFCTEXT)
    Rails/Rail2/@Rail2Name = "Middle" (IFCTEXT)
    Rails/Rail2/@Rail2PartDef = "Circulation::Railing" (IFCLABEL)
    Rails/Rail2/@Rail2Profile = "PIPE1-1/2XS" (IFCTEXT)
    Rails/Rail2/@Rail2ProfileType = "Structural Section" (IFCTEXT)
    Rails/Rail2/@Rail2SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail2/@Rail2TopOffset = 2.5 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail3/@Rail3JoinMethod = "<none>" (IFCTEXT)
    Rails/Rail3/@Rail3Name = "BaseOffset" (IFCTEXT)
    Rails/Rail3/@Rail3PartDef = "Circulation::Railing" (IFCLABEL)
    Rails/Rail3/@Rail3Profile = "PIPE1-1/2XS" (IFCTEXT)
    Rails/Rail3/@Rail3ProfileType = "Structural Section" (IFCTEXT)
    Rails/Rail3/@Rail3SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail3/@Rail3TopOffset = 1.33333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail4/@Rail4JoinMethod = "<none>" (IFCTEXT)
    Rails/Rail4/@Rail4Name = "Lower" (IFCTEXT)
    Rails/Rail4/@Rail4PartDef = "Circulation::Railing" (IFCLABEL)
    Rails/Rail4/@Rail4Profile = "RECT4x1/4" (IFCTEXT)
    Rails/Rail4/@Rail4ProfileType = "Structural Section" (IFCTEXT)
    Rails/Rail4/@Rail4SideOffset = 0.08333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail4/@Rail4TopOffset = 0.33333333333 (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail5/@Rail5JoinMethod = "Vertical" (IFCTEXT)
    Rails/Rail5/@Rail5ProfileType = "<none>" (IFCTEXT)
    Rails/Rail5/@Rail5SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail5/@Rail5TopOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail6/@Rail6JoinMethod = "Vertical" (IFCTEXT)
    Rails/Rail6/@Rail6ProfileType = "<none>" (IFCTEXT)
    Rails/Rail6/@Rail6SideOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]
    Rails/Rail6/@Rail6TopOffset = 0. (IFCLENGTHMEASURE) [foot (conversion based)]